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[bookmark: _top]Control of Substances Hazardous to Health (COSHH) Risk Assessment Form
	Name of substance:
	Glade Pacific Breeze Aerosol

	Other documents to be referenced using this substance:
	Refer to Safety Data Sheet.

	Assessment date:
	07/05/2022

	Review date:
	07/05/2025

	Describe the activity or work process:
(Include how long and how often this is carried out and the quantity of substance used)
	Air care products.

	Identify the persons at risk: (Employees, Contractors, Public, Other – please specify)
	Employees
Contractors

	Name of the manufacturer/supplier:
	SC Johnson Professional Glade

	Concentration:
	Quaternary ammonium compounds, benzyl-C12-16-alkyldimethyl, chlorides>=0.00-<0.10 Butane >=5.00-<10.00 
2-methylbutane >=0.00-<0.10 propane-1,2-diol >=0.00-<0.10 1,3-butadiene >=0.00-<0.10


(A copy of a current safety data sheet for this substance must be attached to this assessment.)
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[bookmark: _Toc94788654]Classification (Category of Danger)
	Danger
	Symbol
	Yes/No/Not Applicable (N/A)

	Flammable
	[image: Flammable Symbol]
	Yes

	Oxidising
	[image: Oxidiser Symbol]
	

	Explosive
	[image: Explosive Symbol]
	

	Irritant/Harmful
	[image: Irritant Symbol]
	

	Environment
	[image: Environmental Toxicity Symbol]
	

	Carcinogenic
	[image: Carcinogenic Symbol]
	

	Corrosive
	[image: Corrosive Symbol]
	

	Toxic
	[image: Toxic Symbol]
	

	Pressurised
	[image: Gas Under Pressure Symbol]
	

	Other – please specify 
	[image: Question Symbol]
	



	Hazard/Precautionary Statements (must be included)

	H223: Flammable aerosol
H229: Pressurised container: may burst if heated.
P102: Keep out of reach of children.
P410+P412: Protect from sunlight. Do not expose to temperatures exceeding 50.C/122F.
P210: Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.
P211: Do not spray and open flame
P251: Do not pierce or burn, even after use



	Hazard Type
	Yes/No/Not Applicable (N/A)

	Gas
	

	Vapour
	

	Dust
	

	Mist
	

	Fume
	

	Dust
	

	Liquid
	

	Solid
	

	Other – please specify
	Aerosol



	Route of Exposure
	Yes/No/Not Applicable (N/A)

	Inhalation
	Yes

	Skin
	Yes

	Eyes
	Yes

	Ingestion
	Yes

	Injection 
	

	Other – please specify 
	



Workplace Exposure Limits (WELs) - Please indicate if not applicable (N/A)
	Short-term exposure (15 minutes)
	N/A

	Long-term exposure level (8 hour Time Weighted Average (TWA))
	N/A


[bookmark: _Toc94788655]Personal Protective Equipment (PPE)
	Item
	Symbol
	If yes – specify type/standard

	Air Fed Helmet
	[image: Air Fed Helmet Symbol]
	

	Face Visor
	[image: Face Visor Symbol]
	

	Goggles
	[image: Goggles Symbol]
	

	Safety Glasses
	[image: Safety Glasses Symbol]
	

	Safety Boots/Shoes
	[image: Safety Boots/ Shoes]
	

	Hand Protection
	[image: Hand Protection Symbol]
	Yes- Nitrile gloves

	Overall
	[image: Overall Symbol]
	

	Apron
	[image: Apron Symbol]
	

	Lab Coat
	[image: Lab Coat Symbol]
	

	Half Respirator
	[image: Half Respirator]
	

	Full Respirator
	[image: Full Respirator Symbol]
	

	Face Mask
	[image: Face Mask Symbol]
	

	Ventilation
	[image: Ventilation Symbol]
	

	Local Exhaust Ventilation
	[image: Local Exhaust Ventilation Symbol]
	

	Used Outside
	[image: Used Outside Symbol]
	

	Other – please specify
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	Contact Type
	Description of First Aid Measures

	Inhaled
	Move to fresh air. 
If breathing is affected, get medical attention.

	Skin Contact
	Rinse with plenty of water. 
Get medical attention if irritation develops and persists.

	Eye Contact
	Rinse with plenty of water. 
Get medical attention if irritation develops and persists.

	Swallowed
	If symptoms persist, call a physician.



	Emergency Measures
	Yes/No/Not Applicable (N/A)

	Is health surveillance required?
	No

	Is training required for this process?
	No

	Fire precautions: What actions will be taken in the event of a fire involving these substance(s)?
	Use extinguishing measures that are appropriate to local circumstances 
and the surrounding environment.
Heating may cause an explosion. 
In case of fire and/or explosion do not breathe fumes. 
Exposure to decomposition products may be a hazard to health.
In the event of fire, wear self-contained breathing apparatus. 
Wear suitable protective clothing and gloves. 
Refer to current EN or National standard as appropriate.

	How should an accidental release/spillage be dealt with?
	Use personal protective equipment. 
Remove all sources of ignition. 
Beware of vapours accumulating to form explosive concentrations. Vapours 
can accumulate in low areas.
Outside of normal use, avoid release to the environment. 
Prevent large amounts of product from entering drains. 
Do not flush into surface water or sanitary sewer system. 
Use appropriate containment to avoid environmental contamination.
If damage occurs to aerosol can: 
Contain spillage, and then collect with non-combustible absorbent material, 
(e.g. sand, earth, diatomaceous earth, vermiculite) and place in container 
for disposal according to local/national regulations.
Clean residue from spill site. 
Dike large spills. 
Use only non-sparking equipment.



[bookmark: _Toc94788657]Storage, Handling, and Other Information
	Handling
	Do not breathe vapours or spray mist. 
Do not use in areas without adequate ventilation. 
Do not puncture. 
Use explosion-proof equipment. 
Keep away from sources of ignition - No smoking. 
Do not spray on a naked flame or any incandescent material. 
Take measures to prevent the build up of electrostatic charge.

	Storage
	No smoking. 
Store in cool place. 
Do not freeze. 
Pressurized container: protect from sunlight and do not expose to 
temperatures exceeding 50 °C. Do not pierce or burn, even after use.
Keep out of the reach of children. 
No decomposition if stored and applied as directed.



	Disposal Method – How should these substances be disposed of (or not disposed of?)
	Yes/No/Not Applicable (N/A)

	Hazardous waste
	

	Skip
	

	Return to depot
	

	Return to supplier
	

	Other (please state)
	Do not dispose of waste into sewer. 
Do not contaminate ponds, waterways or ditches with chemical or used container. 
Disposal should be in accordance with local, state or national legislation. 
Please recycle empty packaging.
Do not re-use empty containers.
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	Assessment completed by:
	The CoSHH Group

	Signature:
	The CoSHH Group

	Date:
	07/05/2022
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